
-Product name:-Square color Camera

Product model:-DV-3125C
Product size:-25x25mm
Image sensor-1/3" Color CCD SONY

Effective Pixels-NTSC : 512(H)X492(V)

 -PAL : 500(H)X582(V)

Resolution-420 TV Lines

Synchronizing system-Internal

Scanning system-NTSC 525 Lines      PAL 625 Lines      2:1 Interlaced

Video output-  1.0Vp-p Composite. 75 Ohms

S/N ratio-More then 48 dB (AGC Off)

Min. Illumination-0.5 Lux / 0.05Lux

Gain Control-Automatic

White Balance-2100ⅹK…8200ⅹK Auto 4dB~30dB
Gamma Characteristic-Auto r=0.45 

Smear Effect-0.005%

Shutter Speed-NTSC : 1/60…1/100,000 sec
PAL : 1/50…1/100,000 sec

Power source-12VDC / 400mA

 Operating current-125mA / regulated 12V DC in

   Lens-Standard-2.5mm,2.97mm,3.6mm , 4mm , 6mm, 8mm Board Lens

 Operating Temperature-14ⅹ F … 122ⅹ F (-10ⅹ C … +50ⅹ C)
Output Terminal- with RCA-Female for Video, DC Jack-Male for Power

Measurement (mm)-25*25mm

Weight (Approx.g)-50g




-Product name:-Super HAD Square color Camera

Product model:-DV-3035CH

Product size:-35x35mm
Specification--
Image sensor-1/3" Super HAD Color CCD SONY

 Resolution-520 TV Lines

Synchronizing system-Internal

Scanning system-NTSC 525 Lines      PAL 625 Lines      2:1 Interlaced

Video output-1.0Vp-p Composite. 75 Ohms

S/N ratio-More then 48 dB (AGC Off)

Min. Illumination-0.5 Lux /0.05Lux
Gain Control-Automatic

Gamma Characteristic-Auto r=0.45 

Smear Effect-0.005%

Shutter Speed-NTSC : 1/60…1/100,000 sec
PAL : 1/50…1/100,000 sec

 Operating current-125mA / regulated 12V DC in

Lens -2.5mm,2.97mm,3.6mm , 4mm , 6mm, 8mm Board Lens

 Operating Temperature-14ⅹ F … 122ⅹ F (-10ⅹ C … +50ⅹ C)
Output Terminal-DIY cable with RCA-Female for Video, DC Jack-Male for Power

Measurement (mm)-35*35mm

Weight (Approx.g)-50g
Prezzi

DV-3125CV 1/3 sony ccd, 25.7mm*25.4mm, 12V DC,23g,  €45.00/pc
DV-3035CH 1/3 sony ccd, 35.4mm*35.2mm, 520TVL, 12V DC, 65g, €60.00/pc
DV-3034CH  1/3 sony ccd, 35mm*34.5mm, 550TVL, 5V DC, about 50g, €52.00/pc 
 
Lens for all 3 items, standard 3.6mm board lens, options: 2.5mm, 2.97mm,4mm,6mm,8mm.
